
The sediment transport model needs the input data from the output of HEC-RAS model. And it contains parallel for-loop, which is setting based on the memory of the author's computer (16 G). Finally, please run the model as the following steps:

1. Run the HEC-RAS model, the model setting files are provided in folder 'HEC-RAS'. Then copy the output files Amm_final.g04.hdf and Amm_final.p07.hdf to this folder.

2. Run the 'Run_script.m', then all output data are stored as .mat files. Users can extract data from these .mat files depending on their interests.