
The files in this folder were created for the Ammer River in SouthWest Germany to obtian the needed hydraulics. Please use HEC-RAS 5.0.0 to read the project and run the model using sediment analysis with quasi-steady flow.

Then please copy the output files Amm_final.g04.hdf and Amm_final.p07.hdf to the folder Sediment_Transport_Model.