Can the implementation of Low Impact Development reduce basin runoff?

Xinxin Sui1,2, Frans van de Ven1,3

1Water Resources Section, Faculty of Civil Engineering and Geosciences, Delft University of Technology, 2628 CD Delft, the Netherlands

2Department of Civil and Environmental Engineering, National University of Singapore, 117576 Singapore, Singapore

3Deltares, 2629 HV Delft, the Netherlands

*Correspondence to*: Frans van de Ven ([F.H.M.vandeVen@tudelft.nl](mailto:F.H.M.vandeVen@tudelft.nl)); Xinxin Sui (SuiXinxin95@163.com)

**Abstract.** Low impact development (LID) was promoted as an alternative to conventional urban drainage methods. The effects of LID at site or urban scales have been widely evaluated. This project aims to investigate the impact of LID implementation on basin runoff at regional scale in a half urbanized catchment; especially the overlap of urban and rural sub-flows at peak times is concerned. A SUPERFLEX conceptual model framework was adapted as a semi-distributed model to simulate the rainfall-runoff relationship in the catchment for San Antonio, Texas as a case study. Scenario analyses of both urban development and LID implementation were conducted. Results show that (1) the infill urban development strategy benefits more from runoff control than the sprawl urban development strategy; (2) in non-flood season permeable pavements, bioretention cells, and vegetated swales decrease peak runoff forcefully and permeable pavements, bioretention cells, and green roofs are good at runoff volume retention; (3) contrary to the general opinion about the peak reduction effect of LID, for partly urbanized, partly rural basins and extremely wet conditions, the implementation of LID practices delays urban peak runoff and may cause stacking of rural and urban sub-flows, leading to larger basin peaks.

# 1 Introduction

Urbanization brought numerous environmental and hydrological changes to river basins and led to severe disturbance to the natural water processes. Unwanted vegetation is removed for urban development, diminishing the vegetation interception and transpiration. Large areas of pervious native soil are replaced by impervious concrete and asphalt for human convenience, impeding runoff infiltration and subsurface water retention. Without sufficient and continuous groundwater recharge, more environmental issues occur, such as land subsidence, groundwater shortage, and water quality degradation (Ahiablame and Shakya, 2016). These human activities modify catchments from a relatively robust natural condition to a sensitive and unstable urbanized status, resulting in water scarcity in dry seasons and waterlogging or urban flooding in rain seasons (Gilroy and Mccuen, 2009; Ahiablame et al., 2012).

To solve flooding problems, the Conventional Drainage approach (CD) is widely exploited in urban areas, which adopts rapid and centralized water transfer strategy: Drainage systems are built to rapidly collect and convey the storm and wastewater from urban impervious areas to centralized municipal facilities, nearby water bodies, or downstream rural areas. The CD approach does not solve water problems such as peak flows and water quality issues, which only shifts the problems to another place to some extent. Low Impact Development (LID) is promoted as an alternative to CD, seeking environmentally friendly solutions for current urban water problems. Instead of conventional centralized grey infrastructures such as pipelines and reservoirs, Low Impact Development exploits blue-green practices such as green roofs and permeable pavements to mimic the natural hydrological system and facilitate rainwater detention and natural purification processes, controlling the rainwater at the source and reducing human impact (Dietz, 2007; Gilroy and Mccuen, 2009; Bedan and Clausen, 2009; Ahiablame et al., 2012; Ulkü et al., 2018).

Since the promotion of the LID concept during the1990s, plenty of LID practices are designed and introduced in different field conditions, to realize diverse hydrological functions and ecosystem services. The most widely used LID practices include (1) Bioretention cells, also known as rain gardens or depressed green, capture runoff with thick layers of soil and lush vegetation. (2) Vegetated swales, shallow and narrow open channels to convey the rainwater, as alternative options for traditional concrete gutters and curbs. (3) Extensive, vegetated green roofs; one of the most popular LID practices because of its claimed advantages, including runoff reduction, house insulation, and ecological and aesthetic benefits. (4) Permeable pavements, a multifunction LID practice, can be flexibly incorporated in different pavement-needed surroundings, enjoying the hydrological benefits of high infiltration and detention capacity.

The effectiveness of LID practices on runoff reduction has been documented by numbers of scientific papers with field tests and simulation investigations. Bioretention cells are shown to reduce 48 % to 97 % of the incoming runoff volume (Chapman and Horner, 2010; DeBusk and Wynn, 2011). For extensive green roofs, the runoff reduction proportion varies a lot between 6.1 % and 100 % with roof slope, media type and depth, vegetation species, and the intensity and duration of rain events (VanWoert et al., 2005; Carpenter and Kaluvakolanu, 2011; Soulis et al., 2017). Hunt et al. (2010) monitored the runoff reduction of a vegetated swale for 23 precipitation events and reported that the runoff reduction proportion has a significant difference between 35 % and 100 % for large and small storm events. Permeable pavements were observed to reduce the runoff between 50 % and 93 % (Rushton, 2001; Hunt et al., 2002; Dreelin et al., 2006). Qin et al. (2013) assessed the performance of swales, permeable pavement, and green roof in a small urbanized basin using the US EPA Storm Water Management Model (SWMM) model and found all three LID practices can retain more flood volume during heavier and shorter storm events. Ahiablame et al. (2016) investigated the runoff reduction under various LID (porous pavement, rain barrel, and rain garden) implementation levels in a highly urbanized watershed with the Personal Computer Storm Water Management Model (PCSWMM) and found runoff reductions from 3 % to 47 %.

While the runoff retention performance of LID practices was extensively documented at the site or urban basin scales, few studies illustrated the influence of LID implementation in a half-rural and half-urbanized catchment at a large scale. This research is necessary, especially for watersheds in which, the urban areas are concentrated close to the outlet. Because of the faster runoff response time of urban lands, there will be a time difference between the urban and rural sub-peaks after a precipitation event. Runoff peaks from the urban part of the basin in most cases reaches the outlet of the basin before the peak of the rural part arrives. However, implementation of LID solutions in city areas may delay the urban sub-runoff and cause more overlap of the urban and rural peaks, and therefore result in a larger basin peak. For downstream flood safety, implementation of LID needs to consider the runoff not only in urban areas but also on the whole catchment scale. That is why, this research aims to study the influence of LID implementation on the basin peaks at a catchment scale.

To investigate the problem of peak stacking of the rural and urban peaks, case study is conducted. The SUPERFLEX conceptual model framework is used to develop a simulation model of the rainfall-runoff relationship of this partly urbanized catchment. Further urbanization of this catchment is foreseen, and to deal with the uncertainty of future urban development, scenario analysis of both LID implementation and urbanization are used to give a reliable answer to the research question. The specific objectives were to (1) investigate the different rainfall-runoff relationships of urban and rural sub-areas; (2) examine the influence of urbanization on the basin runoff; and (3) assess the influence of LID implementation on the basin runoff, especially on the overlap of urban and rural sub-flows at peak times.

The structure of this paper is organized as follows: The study area and data are introduced in Section 2. The methodology about the model setup and scenario design is illustrated in Section 3. The main research results regarding the effects of urbanization and LID implementation on catchment scale are shown in Section 4. Some discussions concerning the limitation of this research and recommendations for future urban development are mentioned in Section 5. And finally, the conclusions are drawn in Section 6.

# 2 Study area, data and modelling tools

## 2.1 Study area

The research catchment is a sub-basin of San Antonio River with 4544 km2. The City of San Antonio takes 27 % of the research catchment (1209.5 km2) and is located near the basin outlet as shown in Fig. 1. Several rivers and creeks, including San Antonio River, flow through San Antonio downtown and then join with Medina River.

San Antonio has a transitional humid subtropical climate featuring hot and humid summers and mild to cool winters. The average annual precipitation is 737 mm. The soil in San Antonio City mainly belongs to moderately permeable clayey soils. Edwards Aquifer is the most prolific groundwater aquifer in the study area, which provides the water for people in San Antonio. To release the stress of the Edwards Aquifer, a groundwater recharge project is developed in the north part of San Antonio by holding back storm runoff in recharge zones. Except for this official groundwater recharge project, managed stormwater infiltration is not allowed in other places, to avoid groundwater pollution (The Edwards Aquifer Website, 2020). Natural stormwater infiltration will inevitably take place in rural and unpaved areas and in LID practices like permeable pavements and bioretention cells. This water will recharge the local groundwater and drains slowly to the river system.

San Antonio has separate foul sewer and stormwater systems. The precipitation collected by the stormwater pipeline system in urban areas is discharged directly to nearby water bodies without treatment. For the wastewater, three major wastewater treatment centers provide water treatment to people in San Antonio and neighboring cities, and the treated water is discharged to nearby rivers (San Antonio Water System, 2020).




Figure 1: The locations of study catchment and two sub-catchments (The rural and urban sub-catchments are colored in green and orange, respectively). The grey areas indicate the City of San Antonio (Colstoun et al., 2017).

As for the social condition, San Antonio city is the seventh most populous city in the U.S. with more than 1.5 million residents (Ready and Montoya, 2019). It is also the fastest-growing of the top ten largest cities in the United States (The City of San Antonio - Official City Website, 2020). From 2010 to 2017, San Antonio experienced a population growth rate between 1.5 % and 2.0 % and the city still keeps a stable demographic expansion. With this stable population increase, the urban land use of San Antonio is expected to grow at a more or less equal pace.

## 2.2 Hydrological data

Retrieved from the USGS website (<https://www.usgs.gov/>), the precipitation, evaporation, and runoff data from study catchment were collected for hydrological modeling of 600 research days, from 2017-04-12 to 2018-12-02. The first 365 days are the calibration period and the last 235 for verification. The time scale is 30 minutes to reflect the fast water response character of urban areas.

Precipitation data from 10 monitoring stations are available, and Thiessen polygons method is used to calculate the total precipitation in this catchment. Evaporation data come from a meteorological station in the research area. The discharge data from three catchments (study catchment and two sub-catchments) are collected from three streamflow monitoring stations as shown in Fig. 1. Among 600 research days, the precipitation and evaporation amounts are 1335 and 1054 mm, and the discharge is 166 mm.

## 2.3 SUPERFLEX model framework

To avoid the drawbacks of too complex models, including high-data requirement, equifinality, and model uncertainty, and to distinguish rural and urban areas in the same catchment, the SUPERFLEX (Fenicia et al., 2011) hydrological modeling framework was adapted to construct a semi-distributed model of this study. The SUPERFLEX modelling framework provides a platform with generic building blocks, such as reservoirs, junctions, and related functions for hydrologists to test dominant water processes and build tailor-made models.

The SUPERFLEX framework was adapted for different topographical conditions (e.g. plateau, hillslope, and wetland), like the FLEX-Topo model (Savenije, 2010). The DYNAMIT (DYNAmic MIxing Tank) model, as promoted by Hrachowitz in 2013, is loosely based on the FLEX model, the predecessor of SUPERFLEX framework. Furthermore, the FLEXG model is a glacier hydrological model, integrated snow and glacier accumulation and ablation processes (Gao et al., 2018). In Lisflood-FP (Hostache et al., 2018) the output of a SUPERFLEX-based model was combined with a hydraulic model to simulate river discharge.

While SUPERFLEX has been used to simulate the rainfall-runoff relationships in different natural landscapes, it has not yet been applied in a highly urbanized catchment. That is why, several urban water processes as well as four LID modules (bioretention cells, green roofs, bioswales, and permeable pavements) had to be formulated and added to the SUPERFLEX framework in this study.

# 3. Methodology

To address the research problem, three urbanization and five LID implementation scenarios are designed to deal with the prediction uncertainty and alternative LID practices. SUPERFLEX conceptual model framework is adapted to a tailor-made semi-distributed model with two hydrological response units (HRUs) for urban and rural surfaces respectively, to simulate the rainfall-runoff relationships of the current situation and the eight scenarios. The scenario design is introduced in this section, following the model setup.

## 3.1 Scenario design

### 3.1.1 Urbanization scenarios

According to the projected urbanization information provided by “City of San Antonio: Comprehensive Plan” (2010), there will be 1.1 million new residents in San Antonio by 2040. Since in this research current time is defined as 2017, expected population growth between 2017 and 2040 is estimated as 0.9 million new residents. The government of San Antonio planned to terminate the unconstrained sprawl of the city but adopt the infill strategy and retrofit existing urban and suburban areas to attract more investment in the urban core and save the high cost of infrastructure and utility services.

Based on the information above, three urban development scenarios for 2040 were designed as shown in Table 1. Scenario A offers an extreme infill urban development situation, in which city size in 2040 will be the same as it is now. Scenario B presents a partial-infill, partial-sprawl urban development situation. In this scenario, 70 % of the new residents will live in current urban areas, while 30 % of new residents will be living in new suburban areas. In scenario C, 50 % of the new residents are assumed to stay in urban expansion areas, while the other 50 % will infill current vacant and underutilized urban areas. Since the infill development strategy may lead to compact living space, per capita living space for scenario A is assumed to be 0.85 times the current areas, and this ratio is 0.9 for scenario B, while no compact living space is assumed for scenario C.

Table 1. Urban development scenarios between 2017 and 2040, based on City of San Antonio: Comprehensive Plan (2010)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Scenarios | Total residents | Percentage of new residents following the infill development [%] | Residents in current urban areas [million] | Percentage of new residents following the sprawl development [%] | Residents in urban expansion areas [million] | Compact factor for living space |
| Current (2017) | 1.5 | - | 1.5 | - | - | - |
| A (2040) | 2.4 | 100 | 2.4 | 0 | 0 | 0.85 |
| B (2040) | 2.4 | 70 | 2.13 | 30 | 0.27 | 0.9 |
| C (2040) | 2.4 | 50 | 1.95 | 50 | 0.45 | 1 |

### 3.1.2 LID implementation scenarios

According to local regulations, the implementation of LID is not strictly mandatory for every development or redevelopment project, and there is great flexibility in the selection of LID practices. Therefore, this research will adopt four most common and typical LID practices to design five LID implementation scenarios based on the conventional urban development scenario C. The first four scenarios assume moderate LID implementations, as 15 % of the precipitation on urban impervious (grey) surfaces will be collected by a single type of LID practice - bioretention cells, vegetated swales, extensive green roofs, and permeable pavement. This will allow us to compare the different hydrological performances of these LID practices.

The last scenario assumes a wide scale LID implementation, as 50 % of the precipitation on urban impervious (grey) surfaces will be conveyed by mixed LID practices (bioretention cells, 15 %; vegetated swales, 15 %; extensive green roof, 5 %; permeable pavement, 15 %), to provide an optimistic and flexible LID implementation plan. Green roofs and permeable pavements serve the area where they are constructed; the ratio of drainage and construction areas of bioretention cells and vegetated swales are 1.5 and 3, respectively, since both collect and retain stormwater from a larger contributing area. Besides, the cascading connections among these LID practices were designed based on realistic construction considerations as shown in Fig. 2.




Figure 2: Cascade connection routes between four LID practices in the mixed LID scenario.

## 3.2 Hydrological model

SUPERFLEX hydrological modeling framework was adapted into a tailor-made semi-distributed model for the San Antonio study catchment. The model’s rainfall-runoff relationship was calibrated and validated with the collected precipitation, evaporation, and runoff data. Based on the current hydrological model, further modifications on water paths were developed for the expression of urban development and LID implementation.

### 3.2.1 Semi-distributed model setup

The hydrological model starts from two simple lumped pre-models, one for a rural and one for an urban sub-catchment, respectively. The dominant water processes were identified from lumped models and inherited by semi-distributed models for the simulation of the whole study catchment. Six generations of semi-distributed models were tested, ranging from six-bucket to eight-bucket (Sui, 2019).

The semi-distributed model was calibrated for a 365-day period on 30-minute scale and then validated with the last 235-day data pairs. A multi-objective calibration approach was exploited in this research: Nash-Sutcliffe Efficiency (NSE) and correlation coefficient (R2) were used to evaluate the modeled time series of runoff. And the frequency domain analysis as quantile-quantile plot (QQ plot) was conducted. Moreover, the runoff characteristics of simulated urban and rural sub-flows were compared with the runoff data collected from the urban and rural sub-catchments. For parameter calibration, the initial range of each parameter was given roughly based on the experience and information about catchment properties according to the physical realism of these parameters (Breuer et al., 2003; Gharari et al., 2014). Then, random parameter sets were sampled between the maximum and minimum limitations with the Monte Carlo method, and more complex models with more parameters were tested with larger numbers of parameter sample sets to ensure the calibration scale as “fair” as possible. For semi-distributed models, two constraints are exploited to reduce the risk of unrealistic combinations of parameters (Hrachowitz et al., 2014; Gharari et al., 2014): (1) the maximum percolation velocity in urban areas is assumed to be smaller than it in rural areas (Pmax,R > Pmax,U). (2) the water storage depth in the unsaturated zone in urban areas is assumed to be smaller than it in rural areas (Sumax,R > Sumax,U).

Table 2. Parameters and model components in the semi-distributed model as shown in Figure 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Description | Model components | Description | Mathematical expression |
| D [-] | Precipitation distribution factor for Su | Pu (mm d-1) | Precipitation on Su |  |
| Ce [-] | Evaporation correction coefficient | Pf/h (mm d-1) | Precipitation on Sf/Sh | / |
| Er [mm d-1] | Reference evaporation | E (mm d-1) | Evaporation |  |
| Sumax [mm] | Maximum unsaturated storage | Qu (mm d-1) | Overflow from Su |  |
| β [-] | Discharge exponent | Pc (mm d-1) | Percolation |  |
| Pcmax [mm d-1] | Maximum percolation velocity | Cr (mm d-1) | Capillary rise |  |
| Cmax [mm d-1] | Maximum capillary rise velocity | Re (mm d-1) | Groundwater recharge |  |
| Rc [1 d-1] | Recharge coefficient | Qp (mm d-1) | Groundwater pumping |  |
| Kh [1 d-1] | Human impact reservoir coefficient | Qs (mm d-1) | Discharge from Ss |  |
| A [mm d-1] | Amplitude of water pumping rate | Qf/h (mm d-1) | Discharge from Sf/Sh |  |
| [-] | Phase of water pumping rate in a day (between 0 and 2π) | △Tlag | Time lag function |  |
| Qpmin [mm d-1] | Minimum water pumping rate |
| Ks/f [1 d-1] | Slow/fast reservoir coefficient |
| α [-] | Discharge exponent |
| Tlag [d] | Time lag coefficient |

The capital letters R or U as subscript in model structure schematic figure indicate Rural or Urban areas, which are not distinguished in this table.

### 

The final selection of the semi-distributed model is a six-bucket model, the schematic figure and mathematical expressions of which are shown in Fig. 3 and Table 2. After the selection of model structure, an appropriate parameter set was selected considering the matching extent of modeled and observed runoff distributions with the quantile-quantile plot (QQ plot) and the model performance in rural and urban sub-catchments.




Figure 3: Schematic figure of semi-distributed model structure. The rural module depicts a fully natural hydrological picture with three reservoirs, including Unsaturated reservoir (SuR), Fast reacting reservoir (SfR), and Slow reacting groundwater reservoir (SsR). The urban module consists of three parts, urban green surface, urban grey surface, and underground parts, corresponding to three reservoirs, Unsaturated reservoir (SuU), Human impact reservoir (ShU), and Slow reacting reservoir (SsU) respectively. The hydrological processes and their mathematical expressions are indicated in Table 2.

### 3.2.2 The expression of urban development in the model

In the semi-distributed model, three urbanization scenarios are expressed with two parameters, 1) the proportion of urban areas in the whole catchment and 2) the proportion of urban grey areas in urban areas (1-D), under the assumption that the degree of urban construction (including water drainage system) and population density are assumed to be consistent in the city. The numerical features of the three urbanization scenarios are shown in Table 3.

Table 3. Parameter calculation table of Urbanization Scenarios

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | *Num.* | *Calculating formula* | Current (2017) | *Scenario* A (2040) | *Scenario* B (2040) | *Scenario* C (2040) |
| Total residents (million) | *(1)* | *-* | 1.5 | 2.4 | 2.4 | 2.4 |
| The residents in current urban areas (million) | *(2)* | *According to scenarios design* | 1.5 | 2.4 | 2.13 | 1.95 |
| The residents in urban expansion areas (million) | *(3)* | *According to scenarios design* | 0 | 0 | 0.27 | 0.45 |
| Per capita urban areas (m2) | *(4)* | *Current urban area / (2)* | 806.3 | 504.0 | 567.8 | 620.3 |
| Expansion areas (km2) | *(5)* | *(3)\*(4)* | 0 | 0 | 153.3 | 279.1 |
| Total urban areas after expansion (km2) | *(6)* | *Current urban area +(5)* | 1209.5 | 1209.5 | 1362.8 | 1488.6 |
| The proportion of urban areas in study catchment | *(7)* | *(6) / Catchment area* | 0.266 | **0.266** | **0.300** | **0.328** |
| Distribution factor of grey areas (1-D) | *(8)* | *Model result for current condition; (9)/(6) for Scenario A, B, C* | 0.170 | **0.232** | **0.218** | **0.221** |
| Total urban grey areas (km2) | *(9)* | *(8)\*(6) for current condition; (10)\*(1) for Scenario A, B, C* | 206 | 280 | 297 | 330 |
| Per capita urban grey areas (m2) | *(10)* | *(9)/(1) for current condition; (10\_current)\*(11) for Scenario A, B, C* | 137 | 117 | 124 | 137 |
| Compact factor of per capita urban grey areas (-) | *(11)* | *Assumption* | 1 | 0.85 | 0.9 | 1 |

The shaded numbers are used to adapt the model for urbanization scenarios A, B, and C

### 3.2.3 The expression of LID practices in the model

The expression of LID in the semi-distributed model follows two procedures. First, the hydrological routes of LID practices were designed and fit in the urban module of the original semi-distributed model. And then, reasonable values were assumed for those involved parameters based on relevant literature, realistic field test results, and data from local government files (Carter and Jackson, 2007; Carter and Rasmussen, 2006; Collins et al., 2008; Hunt et al., 2008; Li et al., 2009; San Antonio River Authority, 2015; San Antonio Water System, 2020; Van Seters et al., 2006;). The schematic model figure of four LID practices in the urban SUPERFLEX module is shown in Fig. 4. The mathematical expressions of hydrological routes and the quantitative comparison of the parameter values are shown in Table 5.




Figure 4: Schematic figure of updated urban model components for four single LID scenarios. (a) In bioretention cells module, Interception reservoir (SiB) and Unsaturated reservoir (SuB) are designed. (b) Permeable Pavement reservoir (SuPP) is added in permeable pavements module. (c) For vegetated swales module, the Vegetated Swales reservoir (SVS) is added. (d) Interception reservoir (SiGR) and Unsaturated reservoir (SuGR) are created for the extensive green roofs module. The LID relevant hydrological processes and their mathematical expressions are indicated in Table 4.

Table 4. Parameters and hydrological routes in LID module. The parameter values of four LID practices are indicated in Table 5.

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Description | Water process | Mathematical expression |
| DLID [-] | Precipitation distribution factor for LID practices | Precipitation on LID practices |  |
| AR [-] | The ratio of the construction area to the drainage area | Evaporation (Interception) |  |
| Ce [mm] | Evaporation coefficient | Effective precipitation after interception |  |
| Er [mm d-1] | Reference Evaporation | Transpiration from LID practices |  |
| Imax,LID [mm] | Maximum interception depth on LID practices | Discharge from vegetated swales |  |
| Sumax,LID [mm d-1] | Maximum water storage depth in subsoil layer of LID practices | Overflow from bioretention cells |  |
| Pcmax [mm d-1] | Maximum percolation velocity | Overflow from green roofs |  |
| SiLID [mm] | The depth of water storage in IR | Overflow from permeable pavements |  |
| SuLID [mm] | The depth of water storage in UR | Percolation from bioretention cells to groundwater |  |
| TlagLID [-] | Time lag coefficient of LID practices | Percolation from vegetated swales to groundwater |  |
| KVS [mm] | Discharge coefficient of vegetated swales | Percolation from permeable pavements to groundwater |  |
| SVS [mm] | Water storage depth in vegetated swales |  |  |
| PcU [mm d-1] | Percolation velocity of urban green areas | Time lag of overflow from LID practices |  |

Table 5. The parameter values of four LID practices

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | DLIDa [-] | ARb [-] | Imax,LID [mm] | Sumax,LID [mm] | TlagLID [-] | KVS [-] |
| Bioretention cell | DB | AR,B≥ 1 | 3.5/AR\*DB | 300/AR\*DB | 13 | - |
| Vegetated swale | DVS | AR,VS ≥ 1 | - | - | 11 | 0.34 |
| Green roof | DGR | 1 | 3.1\*DGR | 42\*DGR | 3 | - |
| Permeable Pavement | DPP | 1 | 4\* DPP | 120\*DPP | 11 | - |

The parameters, DLIDa and ARb, depend on the concrete LID implementation scenarios

# 4. Results

## 4.1 Different hydrological responses of urban and rural areas

The simulated rainfall-runoff relationship under the current condition is shown in Fig. 5, with NSE as 0.68 and R2 as 0.90 during the calibration period and 0.69 and 0.84 during the verification period. The observed total basin runoff is 166 mm in 600 research days. And it is 160 mm for the model result, in which urban districts (27 % of the catchment areas) produce 63 % of total runoff; only 37 % of total runoff is discharged from rural areas (73 % of the catchment areas). In general, rural runoff is more stable than urban runoff. Urban areas generate peak runoff frequently, no matter in dry or rainy seasons, while in rural areas the peak runoffs appear less often with lower peaks.

With the parameter calibration results as shown in Table 6, the different hydrological characters of rural and urban areas can be further explained: First, the precipitation distribution factor for the unsaturated zone (D) and the maximum unsaturated storage depth (Sumax) in the rural module are larger than them in the urban module, which creates larger water retention capacity in rural areas; Second, the larger evaporation coefficient (Ce) in rural areas leads to massive water evaporation, which can be explained by the favorable vegetation condition in rural areas; Third, although the percolation capacity is similar in urban and rural areas with close the maximum percolation velocities (Pcmax), because of the dense vegetation the capillary rise capacity in rural areas is far larger than it in urban areas with higher maximum capillary rise velocity (Cmax); Finally, the value for parameter Ks, indicating the flow rate of deep groundwater, in rural areas is larger than it in urban areas, which indicates a stable and fluent groundwater flow in rural areas. All these four hydrological differences lead to a more stable hydrological performance on peak events for rural landscape than the urban.

Table 6. Parameter values in the current model

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Para. | D [-] | Ce [-] | Sumax [mm] | Pcmax [mm d-1] | Cmax [mm d-1] | Rc [1 d-1] | A [mm d-1] | Qpmin [mm d-1] |
| Rural | 0.98 | 2.7 | 186 | 4.9 | 0.7 | - | - | - |
| Urban | 0.83 | 1.1 | 51 | 4.8 | 0.1 | 1.5 | 0.65 | 0 |
| Para. | beta [-] | Kf/Kh [d-1] | Ks [d-1] | alpha [-] | Tlag [d] | Tlag for rural sub-flow [d] | [-] |  |
| Rural | 6.5 | 0.88 | 0.004 | 8.0 | 1.75 | -0.83 | - |  |
| Urban | 1.6 | 0.51 | 0.002 | 1.5 | 1.75 | - | 2.2 |  |




Figure 5: Model result of the rainfall-runoff relationship in the current simulation. The left and right sides of the red vertical line indicate calibration and verification periods, respectively. (a) indicates the simulated rural and urban sub-flows, and (b) shows the observed and simulated total basin runoff. (b1) and (b2) display the model performance in non-flood and flood seasons respectively.

## 4.2 Urbanization influences on basin runoff

The simulated total runoff volumes and the maximum peak values in 600 research days for the three urbanization scenarios are shown in Table 7. From the view of total runoff volume, all three urbanization plans increased the total basin runoff at different levels. Scenario C, with the highest level of urban sprawl development (50 % of new residents following the infill development) without the compact of per capita living space, brought 14 % additional total basin runoff compared to the current situation. For scenarios B and A, in which 70 % and 100 % of the new residents following the infill development and with the compact factors 0.9 and 0.85, these growth rates are 8.7 % and 2.7 %, respectively.

Table 7. The simulation results of total runoff volumes and the maximum peak runoff values for three conventional urban development scenarios

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Current | Scenario A | Scenario B | Scenario C |
| Total runoff volume in research period [mm] | 160 | 164 | 174 | 183 |
| Increase proportion of the total runoff [-] | - | 2.7 % | 8.7 % | 14 % |
| The maximum peak runoff [mm d-1] | 7.4 | 7.1 | 8.0 | 8.6 |
| Increase proportion of the maximum peak runoff [-] | - | -4.3 % | 7.5 % | 16 % |

As for the peak runoffs shown in Fig. 6, all three urbanization plans brought obvious increases for most peak runoffs in the dry season, among which scenario C always brought the largest peak runoffs followed by scenarios B and A consecutively. But the situation was changed during the rainy season. Fig. 6 (a2) shows three successive basin peaks during flood season. It can be found that urbanization does not necessarily bring higher basin peaks during flood season. This difference is because most basin peaks during non-flood season are mainly generated from urban grey (impermeable) areas, and therefore the peaks will be greatly boosted by the urban development. However, during flood season, the intensive rainfall events fill up the water retention capacity in large areas of rural and urban green (permeable) surfaces. The basin peaks are not only contributed from the urban grey areas but also from large areas of rural and urban green areas. Hence urbanization would not always increase the total basin peaks during flood season.




Figure 6: The simulated total basin runoffs for three urbanization scenarios and current situation. (a1) indicates one basin peak during non-flood season. (a2) shows three successive basin peaks during flood season including the maximum peak event with two summits, I and II. The total runoff volumes and the maximum peak runoff values during 600 research days are displayed in Table 7.

flood,As shown in Fig. 6 (a2), the maximum peak runoff experienced two summits in succession. The lower summit I was mainly contributed by urban grey surfaces with the fast hydrological response after an intense storm event (34.6 mm per hour), and the higher summit II was generated mostly from urban green surfaces accompanied by lighter rainfall. In urbanization scenario A, part of urban green areas was replaced by urban grey areas to meet the needs of population growth, and therefore the runoff of the latter summit II partially moved forward and superimposed on the previous summit I, which causes the decrease of the latter summit II. This phenomenon also occurred on the next two peaks. The faster urban runoff in urbanization scenarios moved far from slow rural peaks and decreased basin peaks compared to them in the current situation.

Overall, the infill urban development strategy is more helpful in basin runoff control for both total volumes and peak values than the sprawl urban development strategy. And secondly, even though urbanization inevitably brings the growth of basin runoff volume, the peak value of total basin runoffs in flood-season can be reduced by adjusting the areas of permeable and impermeable surfaces, as the faster runoff can help to spread the peak over a longer period of time, hence reduce peaks in the total runoff.

## 4.3 LID performance in the non-flood season

The time series of forecast runoff in five LID scenarios and the Conventional urban Development scenario (CD scenario C, following a half-infill and half-expansion urban development strategy) are shown in Fig. 7. Compared to the CD scenario C, all the five LID scenarios significantly reduced most peaks, except for several large peak runoffs happening in flood season around Sep. 2018, which will be discussed in section 4.4.




Figure 7: Comparison of the total basin runoffs in five LID scenarios (blue lines) and the CD scenario C (red line) during 600 research days. The total runoff volumes and the typical peak values are displayed in Table 8. Figure 8 shows a zoom in on the typical peak event happening on 29th Mar. 2018.

The third maximum peak runoff in 600 research days happening on 29th Mar. 2018, non-flood season is selected as the typical peak runoff to further reveal the LID performance on peak runoff reduction in the non-flood season as shown in Fig. 8. Sharing a similar feature with other peak runoffs, the typical peak experiences two times of summit I and II. The LID practices always reduce the first summit more significantly than the second one. This is because the first summit I is mainly generated by urban grey areas with rapid hydrological response, which is the domain of LID practices. However, the second summit II is mainly generated by large areas of urban green surfaces with slow hydrological response, and therefore the LID practices have limited influence on summit II.




Figure 8: The typical total basin peak runoffs happening on 29th Mar. 2018 and the rural sub-flow in five LID and one CD scenarios. The values of summit I and II of the typical peak are illustrated in Table 8

The modelled total basin runoff volume and two summit values of the typical total basin peak runoff in five LID and one CD scenarios are shown in Table 8.

Table 8. The simulation results of total basin runoff volumes in 600 research days and two summit values of the typical total basin peak runoff in six LID scenarios

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Scenarios | CD | Green roof | Vegetated swales | Bioretention | Permeable pavement | Mixed LID |
| Total basin runoff volume [mm] | 182 | 178 | 180 | 178 | 178 | 170 |
| Decrease proportion of the total runoff [-] | - | 2.3 % | 1.0 % | 2.4 % | 2.5 % | 6.9 % |
| Summit I of the typical peak runoff [mm d-1] | 7.3 | 7.0 | 6.8 | 6.7 | 6.6 | 5.3 |
| Decrease proportion of the summit I [-] | - | 4.4 % | 7.6 % | 8.8 % | 9.5 % | 28.3 % |
| Summit II of the typical peak runoff [mm d-1] | 6.48 | 6.47 | 6.50 | 6.39 | 6.34 | 6.26 |
| Decrease proportion of the summit II [-] | - | 0.2 % | -0.2 % | 1.4 % | 2.2 % | 3.5 % |

The specific runoff reduction amounts contributed by each hydrological function in four single LID scenarios are listed in Table 9.

Table 9. Specific urban water balance components in 4 single LID practice scenarios in 600 research days

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | Prec. | Evap. | Infil. | Overflow | Storage |
| Bioretention cell | Amount (mm) | 437 | 94 | 238 | 70 | 35 |
| Ratio | 100 % | 22 % | 55 % | 16 % | 8 % |
| Green roof | Amount (mm) | 437 | 188 | - | 160 | 89 |
| Ratio | 100 % | 43 % | - | 37 % | 20 % |
| Vegetated swale | Amount (mm) | 437 | - | 110 | 328 | 0 |
| Ratio | 100 % | - | 25 % | 75 % | 0 |
| Permeable pavement | Amount (mm) | 437 | - | 383 | 38 | 16 |
| Ratio | 100 % | - | 88 % | 8.6 % | 3.7 % |

### 4.3.1 The performance of bioretention cell scenario

Bioretention cells have significant reduction effects on both total runoff volume and peak runoff values, second only to the permeable pavements. The total basin runoff was reduced by 2.4 % from 182 mm to 178 mm in 600 research days. As for peak values, bioretention cells produced considerable reduction on the summit I of the typical peak with a removal proportion as 8.8 % from 7.3 mm to 6.7 mm , and the robustness of bioretention cells is also satisfactory resulting in a 1.4 % reduction ratio for the summit II.

The strong runoff reduction ability of bioretention cells ascribes to the rapid water infiltration between soil granules and a large volume of water transpiration by lush vegetation. According to the simulation results shown in Table 9, 84 % of the water inflow was reduced by bioretention cells, in which 55 % of the precipitation was infiltrated into the underground, and 22 % and 8 % was evaporated and retained. In the studies of Chapman and Horner (2010) and DeBusk and Wynn (2011), bioretention cells were shown to reduce total runoff volume from 48% to 97%.

### 4.3.2 The performance of permeable pavement scenario

Permeable pavements show the best hydrological performance on basin runoff reduction among the four LID practices. In the permeable pavement scenario, the total runoff volume declined 2.5 % from 182 mm to 178 mm, and the two summits of typical peak runoff were reduced by 9.5 % and 2.2 % respectively. Even though sharing a similar total runoff volume reduction with bioretention cells, permeable pavements better reduced peak runoffs.

In 600 research days, permeable pavements generated the least overflow, only 8.6 % of the total input rainwater, as shown in Table 9. Almost 90 % of the rainwater consumption of permeable pavements depends on the infiltration because additional stormwater retention space is available in the subbase, the base and between the permeable pavers or in the porous asphalt pores. The result is consistent with previous studies, in which permeable pavements consumed 50% to 93% runoff (Rushton, 2001; Hunt, 2002; Dreelin, 2006). Since the large water retention capacity and forceful peak runoff reduction ability, bioretention cells and permeable pavements can be seen as the most effective LID practices for urban flood control and for releasing pressure on the urban drainage system.

### 4.3.3 The performance of vegetated swale scenario

Vegetated swales achieved an appreciable peak runoff reduction similar to bioretention cells and permeable pavements. As shown in Table 8, vegetated swales decreased 7.6 % of the summit I of typical peak runoff. But the sustainability of this peak runoff reduction ability is weak: rather than exhaustively consuming, vegetated swales delayed the runoff of the first summit I till the second one, which caused a larger summit II.

As for the retention of total runoff volume in the long term, the performance of vegetated swales was not outstanding. During 600 research days, only 1 % of the total runoff volume was preserved. For the 437 mm stormwater conveyed by vegetated swales, 75 % of the rainwater was discharged to the urban drainage system, and only 25 % of the total rainfall was absorbed by the soil layer. According to previous studies, the performance of vegetated swales has significant differences between small rainfalls and large storm events. For small rainfall, 85% of the runoff volume can be retained; however, for the large storms, this proportion ranges from 35% to 66% (Hunt, 2010). It can be explained by the fast water transportation mechanism of vegetated swales. Without sufficient water retention capacity, vegetated swales do not support stable and continuous infiltration during large storms. Therefore, the total runoff reduction volume of vegetated swales is distinctly smaller than the other three test LID practices.

### 4.3.4 The performance of extensive green roof scenario

The extensive green roofs brought about the least peak runoff reduction among four test LID practices. Two summits of typical peak runoff were reduced by 4.4 % and 0.2 %, which are far less than in other scenarios. However, the reduction on total runoff volume of green roof scenario is more satisfactory with the reduction ratio as 2.3 %, which is close to this ratio in permeable pavement (2.5 %) and bioretention cell (2.4 %) scenarios. According to the specific runoff retention amount, the water consumption of green roofs relied on evaporation (43 %) and water storage (20 %), while 37 % of the rainwater overflowed. In literature, the runoff reduction capacity of green roofs varies largely between 23% and 100% (VanWoert, 2005; Hathaway, 2008; Carpenter and Kaluvakolanu, 2011).

The significant difference between runoff volume and peak value reductions ascribes to the small water retention capacity of green roofs: Although the green roof shares a similar model structure to bioretention cells with vegetation and soil, the soil thickness of extensive green roofs is small and no infiltration process happen on rooftops. The small water retention capacity of green roofs leads to a sensitive hydrological performance to the predecessor rains: If there are no or fewer predecessor rains, the green roof can still play a role in peak runoff reduction; however, when it comes to rainy seasons, the green roof will be easily filled up by the frequent storm events and lose its peak runoff reduction function.

### 4.3.5 The performance of mixed LID scenario

The mixed LID scenario is the most forceful LID scenario to reduce both the peak runoff and the total runoff volume. The typical peak runoff was decreased considerably in the mixed LID scenario, as 28 % for the submit I and 3.5 % for the submit II. As for the total runoff volume in 600 research days, the mixed LID practices restricted the generation of total basin runoff volume from 182mm to 170mm with a 6.9 % reduction ratio. Except for the large contribution area of LID practices, another advantage of the mixed LID scenario attributes to the cascade connection among LID practices, which adjusts the unbalanced water capture capacities of different LID practices, reinforcing the robustness of the LID system.

Table 10 shows the specific water retention amounts of 4 LID practices in the mixed LID scenario. The evaporation of green roofs and bioretention cells, and the infiltration of bioretention cells and permeable pavements realized abundant water uptakes. In the mixed LID scenario, bioretention cells became the most effective and efficient LID practices among four test LID practices with the largest runoff volume consumption and fewer construction areas. Comparing the hydrological performances of bioretention cells in single bioretention cells and mixed LID scenarios, with more water input and less construction area, the water retention ability of bioretention cells, especially the evaporation, was better developed with almost the same proportion of overflow.

Table 10. Specific urban water balance components of 4 LID practices in mixed LID scenario in 600 research days

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Preca | Inflowb | Evap | Infil | Storage | Overflow | Consume |
| Green roof (5 %) | Amount (mm) | 437 | - | 255 | - | 2.5 | 180 | 257 |
| Ratio | - | - | 58 % | - | 0.6 % | 41 % | 49 % |
| Bioretention cell (15 %) | Amount (mm) | 437 | 60 | 257 | 133 | 25 | 82 | 415 |
| Ratio | 88 % | 12 % | 52 % | 27 % | 5.0 % | 17 % | 84 % |
| Vegetated swale (15 %) | Amount (mm) | 437 | 82 | - | 43 | 0 | 476 | 43 |
| Ratio | 84 % | 16 % | - | 8.4 % | 0 | 92 % | 8.4 % |
| Permeable pavement (15 %) | Amount (mm) | 437 | - | - | 383 | 16 | 38 | 399 |
| Ratio | - | - | - | 88 % | 3.7 % | 8.6 % | 91 % |

Preca and Inflowb indicate the stormwater collected directly by the LID practices and the recharge from other LID practices.

## 4.4 LID performance in flood season

The analysis above concerns the general peak runoffs in non-flood seasons. Fig. 9 shows three basin peaks and their rural and urban sub-flows in flood season. It can be found for the last two peaks dominated by rural runoffs, and all the five LID scenarios lost the peak reduction ability. Table 8 records the specific total basin peak values. It is noticed that except for the third peak happening on 23rd Sep. 2018 in permeable pavements scenario, all the five LID scenarios brought bigger peak values than CD scenario C. And further, the mixed LID scenario, which was supposed to be the most powerful runoff reduction plan, led to peak *increases* of 2 % from 6.35 mm to 6.47 mm and from 3.57 mm to 3.65 mm, which is 2.3 %.




Figure 9: (a) Three successive basin peaks in flood season and (b) their rural and urban sub-flows in five LID scenarios and one CD scenario C. The specific values of the last two basin peaks are shown in Table 11.

Table 11. The values of two basin peaks happening in flood season for five LID scenarios and one CD scenarios

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Scenarios | CD scenario C | Green roof | Vegetated swales | Bioretention | Permeable pavement | Mixed LID |
| Peak runoff in 17th Sep. [mm d-1] | 6.35 | 6.36 | 6.42 | 6.36 | 6.36 | 6.47 |
| Increase proportion [-] | - | 0.1 % | 1.0 % | 0.1 % | 0.1 % | 2.0 % |
| Peak runoff in 23rd Sep. [mm d-1] | 3.57 | 3.58 | 3.60 | 3.58 | **3.56** | 3.65 |
| Increase proportion [-] | - | 0.4 % | 1.0 % | 0.3 % | **-0.1 %** | 2.3 % |

This anomalous condition is triggered by the intensive rainfalls during flood season have exhausted the water retention capacity in rural areas, and therefore these peak runoffs are not only generated from urban areas but also from rural areas. The runoff delay function of LID practices slowed down part of urban peak runoff, which caused stacking of urban and rural peaks and in consequence increased the total basin peak runoff. As the third peak event on 23rd Sep. 2018 shown in Fig. 9, the urban sub-flow occurred two summits generating from urban grey and green surfaces, respectively. The summit I of urban sub-flow in CD scenario C was almost erased by LID practices in mixed LID scenario, but the decreased summit I was partly delayed and superimposed on the summit II, which brought a larger stack of urban and rural peaks and increased the total basin runoff by 2.3 %.

To further confirm LID influences in flood season, ten precipitation events with different rain intensities and durations were selected from the 600-day precipitation observation. These rain events were tested after 15th Sep. 2018 in mixed LID scenario. Among these ten test precipitation events, eight basin peak values were increased from 0.1 % to 3.2 % after the implementation of mixed LID practices, while only two peaks were decreased by -0.2 % and 3.1 %. Especially for three large rainstorms, the peak values increased from 0.75 %, 1.17%, and 1.82%. Even though the increase is small, it is to be concluded that during extremely wet conditions, the effect of implementing LID measures on peak flow reduction is negligible, if not negative in basins with combined urban and rural land use.

# 5. Discussions

## 5.1 Transferability of research results

Since the specific geographical conditions of study catchment, the research results about the growing total basin peaks after LID implementations are limited to restricted regions. The transferability of the result presented here needs to consider the following basin characteristics: To have a risk of stacking of urban and rural peaks after LID implementation . Moreover, sFinally, the extent of LID implementation will quantitatively influence the basin peaks, as a higher degree of LID implementation may bring a larger stack of urban and rural sub-flow in flood seasons.

## 5.2 Limitations

To decrease the model uncertainty caused by over-complex models and to determine a suitable level of model complexity (Hrachowitz et al., 2014), this research used a relatively simple semi-distributed model to simulate the rainfall-runoff relationship on the catchment scale. Heterogeneity within the rural and urban areas is not represented in our semi-distributed model.

Then, important assumptions are used in the urban development and LID implementation scenarios. First, 2.4 million residents are supposed to live in San Antonio City with three compact factors (0.85, 0.9, and 1) for living space in 2040 in three urbanization scenarios. Uncertainty in these figures is high. Next, the extent of urban construction and LID implementation is assumed to be consistent throughout urban areas. However, the construction density of urban core areas might be larger than the new-developed suburban areas. Finally, five LID implementation scenarios presume optimistic LID implementation conditions by using favorable LID parameters, hence overlooking practical implementation, operation, and maintenance problems such as the damage of LID practices and the blockage in soil media. All such limitations lead to discrepancy between the model results and reality. The results however show that the answer to our research question, “[what is] the influence of LID implementation on the basin peaks at a catchment scale” remains valid for different urban development and LID implementation scenarios.

## 5.3 Comparative analysis

The model results about LID performances are also supported by former studies. Firstly, the permeable pavements are considered as the most hydrologically effective LID practices among the four test LID practices. A similar conclusion was also drawn by Ahiablame et al. (2012). Secondly, the ineffective runoff reduction of vegetated swales is ascribed to its fast rainwater transportation and short residence time in this research. Huang (2018) used the same reason to explain the less effective performance of infiltration trenches and vegetated swales compared with bioretention cells, porous pavements, green roofs and etc. . Finally, rather than single LID practices, the mix of various LID practices should be promoted with better robustness. A similar argument was also mentioned by Qin et al. (2013), Askarizadeh et al. (2015), Fang et al. (2017), and Huang et al. (2018).

## 5.4 Recommendations

With regards to urbanization, the infill urban development strategy is recommended for flood control rather than the sprawl urban development strategy. Secondly, although urbanization may inevitably result in the rising of total runoff volume, extreme peak runoffs could be controlled by adjusting the ratio of urban grey and green areas and creating the time differences between the peak runoffs from these sub-areas. However, stacking of peak flows from urban and rural parts of the basin should be avoided by making use of the faster urban runoff versus the slower rural one.

To improve our understanding on total basin peak control, future research can study the hydrological response times of different landscapes. The sub-areas dominated by different land use categories, soil types, topographic conditions, urbanization extents, and their positions in one catchment can be studied. This research assumed homogeneous rural and urban hydrological patterns. Future research could further analyze this problem considering spatially heterogeneous areas, such as partial urban development and uneven LID implementation condition, using distributed models with more precise data supports.

# 6. Conclusions

In this research, a case study for the catchment of San Antonio, Texas was conducted to investigate the influence of LID implementation on the basin runoff at a catchment scale. Scenario analyses of both urban development and LID implementation were adopted to give a reliable answer to the research question. A SUPERFLEX conceptual model was adapted as a semi-distributed model to simulate the rainfall-runoff relationships of study catchment’s hydrological behavior under different scenarios. It was found that:

1. The urban surface, taking 27 % of study catchment, generated 63 % of total basin runoff as 101 mm in 600 research days, while the last 73 % rural areas only produced 37 % of total runoff as 58 mm. And with less water retention capacity urban areas yielded peak runoffs more frequently than rural areas.

2. The infill urban development strategy benefits more from runoff control than the sprawl urban development strategy. All three urban development scenarios brought growth of total runoff volume with increase ratios as high as 14.3 % for scenario C (half-infill and half-expansion urban development plan), 8.7 % for scenario B (70 %-infill and 30 %-expansion), 2.7 % for scenarios A (fully infill development). Fortunately, however, by converting the urban development strategy from urban expansion to infill development, the extreme peak runoff can be reduced from 8.6 mm (scenario C) to 8.0 mm (scenario B) and 7.1 mm (scenario A) that even smaller than 7.4 mm in the current situation.

3. All the five LID implementation scenarios performed powerful runoff reduction ability on the peak runoffs in non-flood seasons. Bioretention cells and permeable pavements can significantly decrease both total basin runoff volume (with the reduction ratios as 2.4 % and 2.5 %) and peak values (8.8 % and 9.5 %). With more water input and less construction area (as the ratio of drainage to the construction area increases from 1 to 1.5), the water retention ability of bioretention cells, especially evaporation, can be better developed with almost the same proportion of overflow. Vegetated swales, without substantial water retention capacity, seem to perform a limited runoff volume reduction (1 %) than the other three LID practices but have satisfactory peak runoff reducing ability (7.6 %). On the contrary, green roofs have the worst peak runoff removal ability (4.4 %) and normal runoff volume reduction capability (2.3 %). The mixed LID scenario provides a forceful solution on runoff reduction as the typical peak runoff was decreased by 28.3 %, and the total basin runoff volume in 600 research days was restricted from 182 mm to 170 mm with a 6.9 % reduction ratio.

4. However, when it comes to flood season, all the five LID scenarios lost the peak reduction ability, and a higher degree of LID implementation leads to larger total basin peak runoffs. This is because the runoff delay function of LID practices slowed urban peaks, which caused more stack of urban and rural sub-flows and thus increased the total basin runoff. Two consecutive peak runoffs happening in flood season rose by over 2 % in the mixed LID scenario.

Data availability: Precipitation, evaporation, and runoff data are available on the USGS website (<https://www.usgs.gov/>). The impervious surface data related to Fig. 1 were retrieved from NASA Socioeconomic Data and Applications Center (SEDAC, <https://sedac.ciesin.columbia.edu/>).

Code availability: Please contact the first author regarding code scripts.

Author contribution: Conceptualization, F.V.; Data curation, X.S.; Formal analysis, X.S.; Funding acquisition, F.V.; Investigation, X.S.; Methodology, X.S.; Project administration, F.V.; Resources, X.S.; Software, X.S., Supervision, F.V.; Visualization, X.S.; Writing—original draft, X.S.; Writing—review & editing, F.V. and X.S. All authors have read and agreed to the published version of the manuscript.

Competing interests: The authors declare that they have no conflict of interest.

# References

Ahiablame, L. M., Engel, B. A., and Chaubey, I.: Effectiveness of Low Impact Development Practices: Literature Review and Suggestions for Future Research, *Water, Air, & Soil Pollution,* *223*(7), 4253-4273, doi:10.1007/s11270-012-1189-2, 2012

Ahiablame, L., and Shakya, R.: Modeling flood reduction effects of low impact development at a watershed scale, *Journal of Environmental Management,* *171*, 81-91, doi:10.1016/j.jenvman.2016.01.036, 2016

Askarizadeh, A., Rippy, M. A., Fletcher, T. D., Feldman, D. L., Peng, J., Bowler, P., . . . Grant, S. B.: From Rain Tanks to Catchments: Use of Low-Impact Development To Address Hydrologic Symptoms of the Urban Stream Syndrome, *Environmental Science & Technology*, *49*(19), 11264-11280. doi:10.1021/acs.est.5b01635, 2015

Bedan, E. S., and Clausen, J. C.: Stormwater runoff quality and quantity from traditional and low impact development watersheds 1, *Jawra journal of the american water resources association*, *45*(4), 998-1008, doi:10.1111/j.1752-1688.2009.00342.x, 2009

Breuer, L., Eckhardt, K., and Frede, H. G.: Plant parameter values for models in temperate climates, *Ecological Modelling*, *169*(2-3), 237-293., 2003

Colstoun, B., C., E., Huang, C., Wang, P., Tilton, J. C., Tan, B., Phillips, J., Niemczura, S., Ling, P.-Y., and Wolfe, R. E.: Global Man-made Impervious Surface (GMIS) Dataset From Landsat. Palisades, NY: NASA Socioeconomic Data and Applications Center (SEDAC). https://doi.org/10.7927/H4P55KKF, 2017

Carpenter, D. D., and Kaluvakolanu, P.: Effect of Roof Surface Type on Storm-Water Runoff from Full-Scale Roofs in a Temperate Climate, *Journal of Irrigation and Drainage Engineering,* *137*(3), 161-169, doi:10.1061/(asce)ir.1943-4774.0000185, 2011

Carter, T., and Jackson, C. R.: Vegetated roofs for stormwater management at multiple spatial scales, *Landscape and Urban Planning,* *80*(1-2), 84-94, doi:10.1016/j.landurbplan.2006.06.005, 2007

Carter, T. L., and Rasmussen, T. C.: Hydrologic Behavior Of Vegetated Roofs, *Journal of the American Water Resources Association,* *42*(5), 1261-1274, doi:10.1111/j.1752-1688.2006.tb05611.x, 2016

Chapman, C., and Horner, R. R.: Performance Assessment of a Street-Drainage Bioretention System, *Water Environment Research,* *82*(2), 109-119, doi:10.2175/106143009x426112, 2010

Collins, K. A., Hunt, W. F., and Hathaway, J. M.: Hydrologic comparison of four types of permeable pavement and standard asphalt in eastern North Carolina, *Journal of Hydrologic Engineering*, *13*(12), 1146-1157, doi: 10.1061/(asce)1084-0699(2008)13:12(1146), 2008

Debusk, K. M., and Wynn, T. M.: Storm-Water Bioretention for Runoff Quality and Quantity Mitigation, *Journal of Environmental Engineering,* *137*(9), 800-808, doi:10.1061/(asce)ee.1943-7870.0000388, 2011

Dietz, M. E.: Low Impact Development Practices: A Review of Current Research and Recommendations for Future Directions, *Water, Air, and Soil Pollution, 186*(1-4), 351-363, doi:10.1007/s11270-007-9484-z, 2007

Dreelin, E. A., Fowler, L., and Carroll, C. R.: A test of porous pavement effectiveness on clay soils during natural storm events, *Water Research,* *40*(4), 799-805, doi:10.1016/j.watres.2005.12.002, 2006

Fang, X., Li, J., Gong, Y., and Li, X.: Zero increase in peak discharge for sustainable development, *Frontiers of Environmental Science & Engineering*, *11*(4). doi:10.1007/s11783-017-0935-5, 2017

Fenicia, F., Kavetski, D., and Savenije, H. H.: Elements of a flexible approach for conceptual hydrological modeling: 1. Motivation and theoretical development, *Water Resources Research*, *47*(11), doi:10.1029/2010wr010174, 2011

Gao, H., Li, H., Duan, Z., Ren, Z., Meng, X., and Pan, X.: Modelling glacier variation and its impact on water resource in the Urumqi Glacier No. 1 in Central Asia, *Science of the total environment*, *644*, 1160-1170., 2018

Gharari, S., Hrachowitz, M., Fenicia, F., Gao, H., and Savenije, H. H.: Using expert knowledge to increase realism in environmental system models can dramatically reduce the need for calibration, *Hydrology and Earth System Sciences,* *18*(12), 4839-4859, doi:10.5194/hess-18-4839-2014, 2014

Gilroy, K. L., and Mccuen, R. H.: Spatio-temporal effects of low impact development practices, *Journal of Hydrology,* *367*(3-4), 228-236, doi:10.1016/j.jhydrol.2009.01.008, 2009

Hathaway, A. M., Hunt,W. F., and Jennings, G. D.: A field study of green roof hydrologic and water quality performance, *Transactions of the ASABE*, *51*(1), 37–44., 2008

Hostache, R., Chini, M., Giustarini, L., Neal, J., Kavetski, D., Wood, M., Corato, G., Pelich, R., and Matgen, P.: Near-Real-Time Assimilation of SAR-Derived Flood Maps for Improving Flood Forecasts, *Water Resources Research*, doi:10.1029/2017wr022205, 2018

Hrachowitz, M., Savenije, H. H., Bogaard, T. A., Tetzlaff, D., and Soulsby, C.: What can flux tracking teach us about water age distribution patterns and their temporal dynamics? *Hydrology and Earth System Sciences,* *17*(2), 533-564, doi:10.5194/hess-17-533-2013, 2013

Hrachowitz, M., Fovet, O., Ruiz, L., Euser, T., Gharari, S., Nijzink, R., Freer, J., Savenije, H. H., and Gascuel-Odoux, C.: Process consistency in models: The importance of system signatures, expert knowledge, and process complexity, *Water Resources Research*, 50(9), 7445-7469, doi:10.1002/2014wr015484, 2014

Huang, C., Hsu, N., Liu, H., and Huang, Y.: Optimization of low impact development layout designs for megacity flood mitigation, *Journal of Hydrology*, *564*, 542-558. doi:10.1016/j.jhydrol.2018.07.044, 2018

Hunt, B., Stevens, S., and Mayes, D.: Permeable Pavement Use and Research at Two Sites in Eastern North Carolina, *Global Solutions for Urban Drainage*, doi:10.1061/40644(2002)39, 2002

Hunt, W. F., Smith, J. T., Jadlocki, S. J., Hathaway, J. M., and Eubanks, P. R.: Pollutant Removal and Peak Flow Mitigation by a Bioretention Cell in Urban Charlotte, N.C, *Journal of Environmental Engineering,* *134*(5), 403-408, doi:10.1061/(asce)0733-9372(2008)134:5(403), 2008

Hunt, W. F., Hathaway, J. M., Winston, R. J., and Jadlocki, S. J.: Runoff Volume Reduction by a Level Spreader–Vegetated Filter Strip System in Suburban Charlotte, N.C, *Journal of Hydrologic Engineering,* *15*(6), 499-503, doi:10.1061/(asce)he.1943-5584.0000160, 2010

Kavetski, D., and Fenicia, F.: Elements of a flexible approach for conceptual hydrological modeling: 2. Application and experimental insights, *Water Resources Research*, 47(11), doi:10.1029/2011wr010748, 2011

Li, H., Sharkey, L. J., Hunt, W. F., and Davis, A. P.: Mitigation of Impervious Surface Hydrology Using Bioretention in North Carolina and Maryland, *Journal of Hydrologic Engineering,* *14*(4), 407-415, doi:10.1061/(asce)1084-0699(2009)14:4(407), 2009

Ready, S. C., and Montoya, A.: SA Climate Ready: A Pathway for Climate Action & Adaptation., Sociology & Anthropology Faculty Research, 52, https://digitalcommons.trinity.edu/socanthro\_faculty/52, 2019

Qin, H. P., Li, Z. X., and Fu, G.: The effects of low impact development on urban flooding under different rainfall characteristics, *Journal of environmental management*, *129*, 577-585, doi: 10.1016/j.jenvman.2013.08.026, 2013

Rushton, B. T.: Low-Impact Parking Lot Design Reduces Runoff and Pollutant Loads, *Journal of Water Resources Planning and Management,* *127*(3), 172-179, doi:10.1061/(asce)0733-9496(2001)127:3(172), 2001

San Antonio River Authority; Bexar Regional Watershed Management’s Low Impact Development Manual Technical Subcommittee, *San Antonio River Basin Low Impact Development Technical Design Guidance Manual*, San Antonio, TX, USA., 2015

San Antonio Water System, Water Recycling: https://www.saws.org/your-water/water-recycling/, last access: 08th Sep, 2020.

Savenije, H. H.: HESS Opinions “Topography driven conceptual modelling (FLEX-Topo)”, *Hydrology and Earth System Sciences Discussions*, 7(4), 4635-4656, doi:10.5194/hessd-7-4635-2010, 2010

Soulis, K. X., Valiantzas, J. D., Ntoulas, N., Kargas, G., and Nektarios, P. A.: Simulation of green roof runoff under different substrate depths and vegetation covers by coupling a simple conceptual and a physically based hydrological model, *Journal of Environmental Management,* *200*, 434-445, doi:10.1016/j.jenvman.2017.06.012, 2017

Sui, X.: The influence of Low Impact Development on rainfall-runoff relationships at catchment scale, Delft University of Technology, the Netherlands, https://repository.tudelft.nl/islandora/object/uuid%3A33776fe7-9428-42c0-9390-fcbb192489fe, 2019

The City of San Antonio - Official City Website: https://www.sanantonio.gov/, last access: 08th Sep, 2020.

The Edwards Aquifer Website: http://edwardsaquifer.net/, last access: 08th Sep, 2020.

Ulkü, M., Sui, X., van der Lans, M., Dillon Peynado, T., Zheng, J., and Fong, C.: Sponge City Project, Multidisciplinary project report, Delft University of Technology, the Netherlands, http://resolver.tudelft.nl/uuid:58200b07-ee01-42e8-8a0f-8881dcda5c07, 2018

Van Seters, T., Smith, D., and MacMillan, G.: Performance evaluation of permeable pavement and a bioretention swale, in: *Proceedings eighth international conference on concrete block paving*, San Francisco, California USA, 6-8 November, 2006

Vanwoert, N. D., Rowe, D. B., Andresen, J. A., Rugh, C. L., Fernandez, R. T., and Xiao, L.: Green Roof Stormwater Retention, *Journal of Environmental Quality,* *34*(3), 1036-1044, doi:10.2134/jeq2004.0364, 2005